[image: ]三角翼組裝檢查表
	VERSION / 版本: V 0.01

	EFFECTIVE DATE / 生效日期: 1 SEP 2026 / 2026年9月1日

	Read & Do / 逐項閱讀並執行

	[ ] = If Applicable / 適用(合格打勾)

	Check clockwise from left to right & from back to front/順時針檢查由左至右由後至前

	1. Basic Information / 基本資訊

	1
	機尾編號/ Tail Number:
	
	Recheck 
☐

	2
	飛行地點(+經緯度)/light Location:
	
	Recheck
☐

	3
	場域大小(飛行場範圍)/ Field size:
	
	Recheck 
☐

	4
	使用空域(+經緯度) /airspace used:
	
	Recheck 
☐

	5
	Date:
日期:
	
	Recheck 
☐

	6
	Time:
時間:
	
	Recheck 
☐

	7
	執行人數:建議3-5人(視機種調整)
	
	Recheck 
☐

	

8
	組裝檢查員/Pre-Flight inspector: 組裝主管姓名/controller Name

技術人員/Technician: 
1. 技術人員姓名/ Technician Name:
2. 技術人員姓名/ Technician Name:
3. 技術人員姓名/ Technician Name:
4. 技術人員姓名/ Technician Name:
5. 技術人員姓名/ Technician Name:
	組裝主管簽名/ Signature of the person who completed the final check:
	



Recheck
☐ 




1
2
3
5
4
6

	2.準備程序(Preperation)

	1
	組裝檢查表需與清單上進度一致(The assembly checklist must align with the schedule on the list.)
	是否嚴格執行(Whether it is strictly enforced)
	☐
confirm
	☐
Unconfirmed

	2
	確認工具與零件規格是否一致(Confirm whether the specifications match)
	是否嚴格執行(Whether it is strictly enforced)
	☐
confirm
	☐
Unconfirmed

	3
	於組裝場地進行組裝(Assembly is carried out at the assembly site.)
	供雙人以上作業使用 (For at least 2 Crew)
	☐
confirm
	☐
Unconfirmed

	4
	組裝工作檯 (TakeOff Table)
	組裝、固定 (Assemble, Secure)
	☐
confirm
	☐
Unconfirmed

	5
	機身根據工作檯標記定位 (Fuselage Positioned According to Table Markings)
	確認 (Confirm)
	☐
confirm
	☐
Unconfirmed

	6
	查看組裝立體圖零附件是否無誤(如上圖)
(Check the assembly diagram and parts/accessories for accuracy.)
	確認 (Confirm)
	☐
confirm
	☐
Unconfirmed







	3.組裝程序(請遵照表格組裝) Assembly procedure (please follow the table for assembly)

	1
	機翼連接桿穿過機身安裝 (Wing Joiners Fitted Through Fuselage)
	確認 (Confirm)
	☐
confirm
	☐
Unconfirmed

	2
	左側機翼連桿連接至機身(The left wing strut connects to the fuselage.)
	確認 (Confirm)
	☐
confirm
	☐
Unconfirmed

	3
	左側側翼連桿連接至機翼(The left-side flank link connects to the wing.)
	確認 (Confirm)
	☐
confirm
	☐
Unconfirmed

	4
	機頭連桿連接至機身(The nose section connects to the fuselage via a connecting rod.)
	確認 (Confirm)
	☐
confirm
	☐
Unconfirmed

	5
	右側機翼連桿連接至機身(The right-side wing strut connects to the fuselage.)
	確認 (Confirm)
	☐
confirm
	☐
Unconfirmed

	6
	右側側翼連桿連接至機翼(The right-side flank link connects to the wing.)
	確認 (Confirm)
	☐
confirm
	☐
Unconfirmed

	7
	左側機翼伺服機馬達接頭(Left wing servo motor connector)
	已連接、交叉檢查 (Connected, Crosschecked)
	☐
confirm
	☐
Unconfirmed

	8
	右側機翼伺服機馬達接頭 (Right-wing servo motor connector)
	已連接、交叉檢查 (Connected, Crosschecked)
	☐
confirm
	☐
Unconfirmed

	9
	左側機翼螺絲(Left wing screw)
	緊固 (Fasten)
	☐
confirm
	☐
Unconfirmed

	10
	右側機翼螺絲(Right-side wing scre)

	緊固 (Fasten)
	☐
confirm
	☐
Unconfirmed

	11
	左側三角翼下連桿確認:長度是否與機翼平行(Left-side delta wing lower link verification: Check if the length is parallel to the wing.)
	已組裝裝上 (Assembled)
	☐
confirm
	☐
Unconfirmed

	12
	左側機翼伺服機馬達點位是否正確(Is the position of the left wing servo motor correct)
	連接 (Connect)
	☐
confirm
	☐
Unconfirmed

	13
	右三角翼下連桿確認:長度是否與機翼平行(Right delta wing lower link verification: Check if the length is parallel to the wing)
	已組裝裝上 (Assembled)
	☐
confirm
	☐
Unconfirmed

	14
	右側機翼伺服機馬達點位是否正確(Is the position of the right-wing servo motor correct)
	連接 (Connect)
	☐
confirm
	☐
Unconfirmed

	15
	機頭螺絲(Pan-head screw)
	緊固 (Fasten)
	☐
confirm
	☐
Unconfirmed

	16
	無刷馬達是否安裝正確(Is the brushless motor installed correctly)
	確認 (Confirm)
	☐
confirm
	☐
Unconfirmed

	17
	無刷馬達螺絲(Brushless motor screws)
	緊固 (Fasten)
	☐
confirm
	☐
Unconfirmed

	18
	馬達槳葉(Motor propeller blades)
	已安裝固定 (Installed)
	☐
confirm
	☐
Unconfirmed














	4.一般機體外觀檢查(GENEAL)

	1
	左側機翼結構 (LH Wing)
	無損壞、乾淨無阻 (Clear)
	☐
confirm
	☐
Unconfirmed

	2
	右側機翼結構 (RH Wing)
	無損壞、乾淨無阻 (Clear)
	☐
confirm
	☐
Unconfirmed

	3
	起落架結構 (Undercarriage)
	無損壞、乾淨無阻 (Clear)
	☐
confirm
	☐
Unconfirmed

	4
	機身主體結構 (Fuselage)
	無損壞、乾淨無阻 (Clear)
	☐
confirm
	☐
Unconfirmed

	5
	所有防護罩/保護蓋(All protective shields/covers)
	已確認安裝固定(Installed)
	☐
confirm
	☐
Unconfirmed

	6
	空速管(Pitot tube)
	已確認安裝固定(Installed)
	☐
confirm
	☐
Unconfirmed

	7
	GPS
	已確認安裝固定(Installed)
	☐
confirm
	☐
Unconfirmed

	8
	無刷馬達(Brushless motor)
	已確認安裝固定(Installed)
	☐
confirm
	☐
Unconfirmed

	9
	馬達槳葉(Motor propeller blades)
	已確認安裝固定(Installed)
	☐
confirm
	☐
Unconfirmed

	10
	酬載確認是否已固定及配重是否達標(Verify that the payload is secured and the counterweight meets the required specifications)
	確認 (Confirm)
	☐
confirm
	☐
Unconfirmed





— 檢查表全項結束 (END OF CHECKLIST) —
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